<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="97.76341427914934" y2="0" width="0" layer="20"/>
<wire x1="97.76341427914934" y1="0" x2="97.76341427914934" y2="101.78259153175105" width="0" layer="20"/>
<wire x1="97.76341427914934" y1="101.78259153175105" x2="0" y2="101.78259153175105" width="0" layer="20"/>
<wire x1="0" y1="101.78259153175105" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="Tinkercad">
<packages>
<package name="LEDRD254W60D565H860B"><description>Radial LED (Round), 2.54 mm pitch, 5.65 mm body diameter, 8.60 mm body height
&lt;p&gt;Radial LED (Round) package with 2.54 mm pitch (lead spacing), 0.60 mm lead width, 0.50 mm lead thickness, 5.65 mm body diameter and 8.60 mm body height&lt;/p&gt;</description></package>
<package name="LEDRD254W60D565H860B_Y"><description>Radial LED (Round), 2.54 mm pitch, 5.65 mm body diameter, 8.60 mm body height
&lt;p&gt;Radial LED (Round) package with 2.54 mm pitch (lead spacing), 0.60 mm lead width, 0.50 mm lead thickness, 5.65 mm body diameter and 8.60 mm body height&lt;/p&gt;</description></package>
<package name="LEDRD254W60D565H860B_G"><description>Radial LED (Round), 2.54 mm pitch, 5.65 mm body diameter, 8.60 mm body height
&lt;p&gt;Radial LED (Round) package with 2.54 mm pitch (lead spacing), 0.60 mm lead width, 0.50 mm lead thickness, 5.65 mm body diameter and 8.60 mm body height&lt;/p&gt;</description></package>
<package name="ARDUINO-UNO-R3-SHIELD"><description>&lt;h3&gt;Arduino Uno-Compatible Footprint&lt;/h3&gt;
No holes, no ICSP connections.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 32&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:2.1x2.35"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Arduino Uno R3 Shield&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description></package>
<package name="RESAD1016W63L850D250B"><description>Axial Resistor, 10.16 mm pitch, 8.50 mm body length, 2.50 mm body diameter
 &lt;p&gt;Axial Resistor package with 10.16 mm pitch (lead spacing), 0.63 mm lead diameter, 8.50 mm body length and 2.50 mm body diameter&lt;/p&gt;</description></package>
</packages>
</library></libraries>
<attributes/>
<variantdefs/>
<elements>
<element name="R3" library="Tinkercad" package="RESAD1016W63L850D250B" value="1k"/>
<element name="D5" library="Tinkercad" package="LEDRD254W60D565H860B_Y" value="YELLOW">
<attribute name="CATEGORY" value="Opto-Electronic"/>
<attribute name="COLOR" value=""/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="LED"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE" value="LED_YELLOW"/>
</element>
<element name="R1" library="Tinkercad" package="RESAD1016W63L850D250B" value="1k"/>
<element name="U2" library="Tinkercad" package="ARDUINO-UNO-R3-SHIELD" value="ARDUINO-UNO-R3-SHIELD"/>
<element name="D4" library="Tinkercad" package="LEDRD254W60D565H860B" value="RED">
<attribute name="CATEGORY" value="Opto-Electronic"/>
<attribute name="COLOR" value=""/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="LED"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE" value="LED_RED"/>
</element>
<element name="R2" library="Tinkercad" package="RESAD1016W63L850D250B" value="1k"/>
<element name="D6" library="Tinkercad" package="LEDRD254W60D565H860B_G" value="GREEN">
<attribute name="CATEGORY" value="Opto-Electronic"/>
<attribute name="COLOR" value=""/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="LED"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE" value="LED_GREEN"/>
</element>
</elements>
<signals>
<signal name="D5_C">
<contactref element="D5" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="U2_D12">
<contactref element="R3" pad="2"/>
<contactref element="U2" pad="D12"/>
</signal>
<signal name="U2_TX">
<contactref element="D5" pad="1"/>
<contactref element="U2" pad="TX"/>
</signal>
<signal name="D4_C">
<contactref element="D4" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="U2_D11">
<contactref element="R1" pad="2"/>
<contactref element="U2" pad="D11"/>
</signal>
<signal name="U2_D13">
<contactref element="R2" pad="2"/>
<contactref element="U2" pad="D13"/>
</signal>
<signal name="U2_D2">
<contactref element="D4" pad="1"/>
<contactref element="U2" pad="D2"/>
</signal>
<signal name="U2_RX">
<contactref element="D6" pad="1"/>
<contactref element="U2" pad="RX"/>
</signal>
<signal name="D6_C">
<contactref element="D6" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>